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	Racking Inspection Checklist
Regular visual check
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	Racking Inspection Checklist · HSIL-FRM-007

	




	Site and location
	
	Inspected by
	
	Date

	
	
	
	
	

	

	Area or run inspected

	


Tick OK, or grade the damage. Green: within limits, monitor. Amber: do not reload once emptied, repair within four weeks. Red: offload and isolate at once.

	Check
	OK
	Green
	Amber
	Red
	Bay and notes

	Uprights: no dents, bends or splits
	
	
	
	
	

	Bracing: straight, all bolts present
	
	
	
	
	

	Uprights: plumb in both directions
	
	
	
	
	

	Base plates and fixings: tight, sound
	
	
	
	
	

	Beams: straight, connectors undamaged
	
	
	
	
	

	Beam locks: fitted at both ends
	
	
	
	
	

	Guards and barriers: in place, sound
	
	
	
	
	

	Load notices: displayed and correct
	
	
	
	
	

	Loads: within capacity, evenly spread
	
	
	
	
	

	Pallets: sound, no overhang
	
	
	
	
	

	Aisles and gangways: clear
	
	
	
	
	

	Decking and accessories: secure
	
	
	
	
	



	Action required

	

	

	Reported to
	
	Signature
	
	Next check due

	
	
	
	
	


This checklist supports a regular visual check. It does not replace an expert inspection, which should be carried out at least every 12 months.
Hull Storage & Interiors Limited · Registered in England and Wales no. 02780524 · VAT no. GB 765 346 017	Page  of 
Reg. office: 57 Spyvee Street, Hull, HU8 7JJ · 01482 218060 · hsil.uk · hsil.co.uk	HSIL-FRM-007 · v1.0 · 01/10/2026
Hull Storage & Interiors Limited · Registered in England and Wales no. 02780524 · VAT no. GB 765 346 017	Page  of 
Reg. office: 57 Spyvee Street, Hull, HU8 7JJ · 01482 218060 · hsil.uk · hsil.co.uk	HSIL-FRM-007 · v1.0 · 01/10/2026
c0fa0779cb19eec3c4ac965c2089cbbb13d9a0c2.png




